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General
· Update all AutoCAD pages (convert to Word documents and follow the updated Wiki Organization Guide)
· Archive old files from the design part of the wiki

· Create a new wiki page with a series of tables of designs showing the variety of designs that can be created by the ADT. Parameters to vary are Q.Plant (5 L/s, 10 L/s, 25 L/s, 50 L/s, 100 L/s), N.SedTanks of 2 for the 5 L/s otherwise increase to 3 or more for large plants, N.SedBayEst (1 for small flows, increase as the flow increases and try different numbers of bays for larger flows to vary the plant layout). For each design, list the input parameters from the online ADT in a table and then provide links to the AutoCAD, xls, and PDF documents.
· Teach the variable naming guide to new members and create a quiz to test comprehension. Each level of the variable description should be getting more specific. The first letter or pair of letters determines the units of the variable. For example which of these is correct? D.SedOrificeDrain (incorrect because the orifice doesn’t have a drain, the drain has an orifice!) or D.SedDrainOrifice (correct)
· Review the methods used to draw plant components. Evaluate the possibility of creating higher level functions for drawing objects. These functions should handle creating the layers, freezing other layers, if necessary subtracting from a different layer (for pipes). The functions should be intuitive to use and generic. They should be created using lower level MtA functions. We need to draw more plant piping and thus creating easy to use piping algorithms would be VERY useful.  
Online AguaClara Design Tool

· Add language specific email responses that include the requirement that the design be reviewed by a professional engineer and that Cornell is not liable for any damages due to the design. These could be simple text files with a naming convention that includes the identifying number of the language (English is 0, Spanish is 1)

· Review input parameters. Consider adding the slab thickness as a separate input parameter.

· Assuming that filtration will be added soon, create a strategy for how the filtration design will be accomplished. 
· Should there be an option for designing individual unit processes rather than always designing the entire plant?

· Considering adding an option for specifying the length of a flocculator channel. Handle this parameter in the same way that the depth of the flocculator is handled. 

Design Review (Error Testing – contact Julie Pierce for guidance)
· Create a MathCAD document that executes at the end of the design process (at the bottom of the list of references in the master program)

· Devise a series of independent calculations (with equations that don’t rely on ANY other MathCAD files) to check the design
· One goal is to create an error message explaining what went wrong if the design tool produces a design that is incorrect or if there are variables that are out of range. This error message would be returned to LabVIEW and included in the email to the client.
· Design checks would include

· Energy dissipation rate in the flocculator

· Collision potential based on total flocculator head loss, flocculator residence time, collision potential efficiency based on H/S.
· Head loss through the launder orifices
· Head loss in the waste channels

· Energy dissipation rate in the inlet manifold ports

· The design checks could also be used to calculate parameters that are reported to the client in the specifications document.

Plant Design for Operator Access

Draw the walkways and any necessary stairs at appropriate elevations so it is easy for the operator to access plant controls. Make sure the operator can easily access the CDC and the chemical stock tanks as well as the tank drain valves. The walkways should be quite high (perhaps 50 cm below the tank walls) on the upper side of the plant near the chemical stock tanks. The walkway covering the drain canal could be at the same high elevation or it could be lower and hence closer to the drain valves. The operator must be able to control the valves and observe the sludge/water exiting into the drain canal from the walkway. Perhaps this walkway needs to be built using a metal grate so the operator can see the drain.
The stock tanks need to be accessible for filling with water and chemicals and for stirring.

There needs to be a place to fill a bucket with clean water from the exit channel. This should be a 1.5 inch pipe through the wall with a valve. The walkway must be low enough so that the bucket fits under this valve.
Entrance Tank 
Add a drain for the entrance tank that can be opened by pulling a pipe nipple (that protrudes through the water surface) out of a coupling embedded in the entrance tank slab.
Entrance Tank Coordination with CDC
Determine if the CDC is going to continue to be positioned directly on top of the entrance tank or if there is a method to move the dosing half of the lever off to the side to reduce the risk of spills into the entrance tank and to make the CDC more accessible.

If the CDC continues to fit directly on top of the Entrance Tank, then make sure that the entrance tank is wide enough for the CDC to fit. Devise means for the CDC to fit on larger entrance tanks for larger flows.
Entrance Tank/Rapid Mixer
Low Flow Rapid Mix Design
· Create a micromix orifice interface on the coupling.
· Create a method to adjust the total head loss through the plant by adding more small orifices to the orifice plate. This is necessary 

· Determine how to 

High Flow Rapid Mix Design

For plant flows that require rapid mix pipes larger than 8 inches in diameter it probably makes more sense to build the 
Chemical Storage Tanks

· Draw tank outlets, which should be located 10 cm above the base of the tank to allow for sedimentation.
· Add dimension calculations for the chlorine stock tanks to the “ChemStorageTanks” MathCAD file. The existing algorithm to calculate Alum stock tank dimensions can be useful to figure out how to do this.

· Edit “Chlorinestock” in the “AutoCAD Scripts” folder so that it draws the stock tanks (refer to the “Alumstock” file that contains design algorithm for the alum stock tanks). Note that the chlorine tanks can be located lower than the alum tanks since the chlorine is applied in the exit channel. If we set the chlorine tanks lower, then it won't be possible to prechlorinate. 

·  Draw pipes connecting the storage tanks to the float valve.

· Include a T in a horizontal section of the line with a drain valve that can be used as a sediment trap to reduce the amount of sediment that gets to the float valve orifice

·  Add ability for the user to input stock concentration, max alum dose, and minimum tank duration to calculate the size of the tanks 

· Add drain lines connected to the very bottom center of the tanks that go to the drain line for the entrance tank and ultimately to the plant drain channel

Automated Plotting

· Finish debugging the new MtoATranslator.
· Update the Mathcad design scripts with the new commands in the MtoATranslator.
· Determine how to put dimensions the paper space using keyboard commands.
· Add text-related commands in the MtoATranslator.
· Find a way to create and edit multiple view ports in one layout. 

 

Launders

· Launder joint at exit channel end needs to be updated to a flexible joint: a short piece of tubing will extend out of the coupling in the wall which will connect to the flexible rubber coupling connecting to the launder. This will allow the launder to extend across the length of the sedimentation tank.

· Code and place small concrete ledges on the inlet channel wall of the sedimentation tank to support each of the launders.

· Couplings are currently drawn to a user-specified length, but in reality come only in certain lengths. Research on McMaster to find coupling sizes, add to pipe database and update so function calls pre-specified lengths. (Did this change?)
· Update all couplings to coupling subtract function so we do not have to keep both files/functions.
Drain Channel
· Code the entire drain channel along the inlet channel side of the sedimentation tank.
· Draw elbow attached to the inlet tee that empties waste water directly into drain channel. Elbow should be angled at 45 degrees so that waste water shoots down the channel in the direction of the flow.
Weir Tanks
· Make tanks be drawn so that they are just an extension of the inlet and exit weir tanks so they can be built as just two long channels. Basically, extend the inlet and exit channels so that they continue to length of weir tanks and add a wall at the end of each channel.
Debugging
· Fix lamina code error for newly designed lamina so that the "purple circles" are no continuously drawn when the code is used by the ADT.

· Fix chimney stops error that occurs for flow rates greater than 32 L/s when used by the ADT. (I think this was fixed?)
Documentation

· Fix flocculator section in the design document. We want to change the field code so that it automatically displays text corresponding to either vertical or horizontal flocculators (whichever is appropriate to the design generated by the design tool). Then, if a vertical flocculator is chosen, we want it to display information about either plastic or rigid baffles (again, whichever is appropriate)

· Integrate the materials list into the design document.

· Integrate costs and management (of AguaClara plants) into the design document.

· Tweak process drawing - make sure that Monroe can use it for CEE 4540 (Sustainable Small-Scale Water Supplies) class. Make sure to update the Lo-text and Hi-text versions.
Plate Settler Support Frame
· Add holder supports in between bays to provide stability for the mainframe.

· Add stubs along vertical pipes to provide stability to the plate settler modules.
