Inlet Manifold Challenges for Fall 2010

We will conduct tests on the uniformity of flow from constant diameter ports with a much smaller hydraulic system (perhaps 1/2" diameter pipe instead of 6") and with much higher flow velocities to make it possible to measure the pressure changes in the manifold pipe using pressure sensors.

