
[image: image4.png]



[image: image2.png]



[image: image3.png]




1. Allows the operator to remove settled flocs from the sedimentation tank

2. A pipe with many holes that removes clarified water from the top of the sedimentation tank. The launder empties into the sedimentation tank exit channel.
3. Regulates the amount of alum (aluminum sulfate) that mixes with the raw water to ensure proper floc formation
4. Transfers flocculated water from the floc tank to the sedimentation tank inlet manifold.

5. The means by which clarified water goes to the filters

6. Process that uses sand filtration to remove small flocs that were not captured by the sedimentation tank. The filter contains several inlet and outlet manifolds to maximize the amount of water filtered per area

7. Series of pipes that distributes clarified water evenly into the packed sand bed
8. Tank with a series of 180-degree turns that generate turbulence that causes collisions between suspended particles; the particles stick together to form flocs if the chemical coagulant dose is correct.
9. Raw water enters the plant here
10. Addition of chlorine to kill any bacteria remaining in the water

11. Series of pipes that removes filtered water from the packed sand bed

12. Tank where flocs settle out of the water

13. Distributes flocculated water evenly throughout the bottom of the sedimentation tank 
14. Reduces the distance a particle has to fall before it is “captured,” or has to fall before it hits a solid surface
15. Contains an orifice or a set of orifices to ensure the chemical coagulant is distributed evenly throughout the water
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