Challenges Chemical Dose Controller Spring 2011
Assess the feasibility of using multiple parallel tubes for the linear doser as a method to extend the range to higher plant flow rates.
Provide guidance on the plant flow rate at which we should switch from linear to non linear dose control.

Could plants be designed to be easily switched from linear to nonlinear dosing?
