Fabrication Team challenges

· Determine best way to attach vertical pipes to the inlet manifold. Experiment with number and size of "legs" formed from boiled PVC (see past work), flanges made from pieces of 6" PVC, or any other methods. Glue on to 6" PVC and measure shear force required to break.

· Take apart old handheld drill battery pack to see if terminals can be connected to a car or deep-cycle battery. Need a 12-gauge wire of 4-5 meters in length. Test drill runtime and drilling power.

· Consider making a frame for a drilling jig that would align plate settlers for easy and accurate drilling. Frame can have pre-drilled holes (use drill press) to make it easy to use.
