PREFABRICATABLE OVEN PRELIMINARY DESIGN 

BASE/OUTER WALLS










WOODEN CORNERS/INNER WALLS TOP VIEW





FRONT VIEW 







TOP COMBINED VIEW 












COVER /TOP VIEW                                                           COVER /SIDE VIEW WITHOUT FRONT WOOD PIECE

		







NOTES: 
MATERIALS COLOR CODE:
GRAY:  INSULATION
WHITE: SHEET METAL
ORANGE: WOOD
LIGHT BLUE: GLAZING
WHITE: SHEET METAL
· DOTTED LINES INDICATE INNER WALL. THE INNER WALL WILL BE INSERTED INTO SLOTS IN THE WOOD CORNERS
· TOP COVER WILL BE DESIGNED SUCH THAT EITHER GLASS OR PLASTIC BAGS CAN BE USED. PLASTIC BAGS WILL BE APPLIED TO A METAL WIRE FRAM AND INSERTED INTO THE SLOT LIKE A PIECE OF GLASS WOULD. (Alternatively, one plastic layer could be placed on top of the oven, the wooden frame is then put on, and finally a top plastic layer is added to the oven with an elastic cord. )
· DIMENSIONS: 20 x 25 x 11 INCHES
Glazing materials: 
· Oven bags, glass, soda bottles  

OTHER IDEAS WE ARE LOOKING INTO: 
· Rigid insulation/foam board/isocyanurate material. Use insulation as structure to create the oven, thus eliminating the need for a frame. “walk in fridge” concept
· Open air, reflector panel cooker. 

[bookmark: _GoBack]Course of Action:
· Create CAD plan with dimensions
· Test plastic bags
· Build prototype  

