*HEADING
ABAQUS job created on 27-Sep-2011 16:14:45
**
*NODE
**
**
*ELEMENT, TYPE=C3D8, ELSET=PROP1
*ELEMENT, TYPE=C3D8, ELSET=PROP1
*ELEMENT, TYPE=C3D8, ELSET=PROP1
**
*SOLID SECTION, ELSET=PROP1, MATERIAL=MAT1
   1.0000000,
**
*MATERIAL, NAME=MAT1
*ELASTIC, TYPE=ISO
   0.2000000,   0.3000000
**
*NSET, NSET=FIXED
*NSET, NSET=ROLLER
*NSET, NSET=COMPRESS
**
**
*PREPRINT, ECHO=YES, MODEL=YES
**
** Displacement boundary condition
*BOUNDARY, TYPE=DISPLACEMENT,OP=NEW
FIXED,       1,,           0
FIXED,       2,,           0
FIXED,       3,,           0
ROLLER,       3,,           0
*STEP, AMPLITUDE=RAMP, PERTURBATION
*STATIC
**
** Applied strain
*BOUNDARY, TYPE=DISPLACEMENT,OP=MOD
COMPRESS,       3,,  -0.0034650
**
**
*NODE FILE, FREQUENCY=1
U,
RF,
CF,
*NODE PRINT, NSET=FIXED, FREQUENCY=1, SUMMARY=YES,TOTALS=YES
RF,
*NODE PRINT, NSET=ROLLER, FREQUENCY=1, SUMMARY=YES,TOTALS=YES
RF,
*NODE PRINT, NSET=COMPRESS, FREQUENCY=1, SUMMARY=YES,TOTALS=YES
CF,
*NODE PRINT, FREQUENCY=1, SUMMARY=YES, TOTALS=YES
U,
*EL FILE, DIRECTIONS=YES, POSITION=INTEGRATION POINTS, FREQUENCY=1
S,
E,
ENER,
*EL PRINT, POSITION=CENTROIDAL, FREQUENCY=1
S,
E,
*EL PRINT, POSITION=CENTROIDAL, FREQUENCY=1
ENER,
*EL PRINT, POSITION=CENTROIDAL, FREQUENCY=1
SP,
EP,
***
*PRINT, FREQUENCY=1
***
*END STEP