Transition Flow Rates

	Description
	Upper Constraint
	Min Q
L/s
	Max Q
L/s

	Pre-fab plants
	Number of pre-fab plants needed, beyond 4.9 L/s, use EStaRs design with sed tanks
	1
	4.9

	2 EStaRS
1 sed tank with room for more sed tanks (include sed inlet and outlet channels when building)
	A bigger sed tank (inlet manifold length of 3.5m) could be used at 7.5 L/s
	5
	<7.5

	2 EStaRS or more
2 sed tanks
	The masonry needed for the filter box for OStaRs gets too difficult (too small for a normal sized person to maneuver) below 16 L/s.
	7.5
	16

	2 or more OStaRS
	Due to a 24in LFOM (biggest pipe size in database)
	16<
	150

	Multiple treatment trains (multiple chemical dosing, entrance tanks, flocculators)
	
	150
	1000







