Partial Differential Equation Toolbox |

assema

Assemble area integral contributions

Syntax

-     [K,M,F]=assema(p,t,c,a,f)
      [K,M,F]=assema(p,t,c,a,f,u0)
      [K,M,F]=assema(p,t,c,a,f,u0,time)
      [K,M,F]=assema(p,t,c,a,f,u0,time,sdl)
      [K,M,F]=assema(p,t,c,a,f,time)
      [K,M,F]=assema(p,t,c,a,f,time,sdl)

Description

`[K,M,F]=assema(p,t,c,a,f)` assembles the stiffness matrix `K`, the mass matrix `M`, and the right-hand side vector `F`.

The input parameters `p`, `t`, `c`, `a`, `f`, `u0`, `time`, and `sdl` have the same meaning as in `assempde`.

See Also

`assempde`

| adaptmesh |  | assemb |