Top

How to use the Mapping Mesh Toolbox

The GUI figure is divided into three main areas: grid creation, subdomain creation, and axes. The grid creation area must be used first. All subdomain vertex locations will snap to grid points.
After creating a grid, you are able to draw a subdomain, alter its vertex locations, and choose the number of divisions along each side.
All drawing and visualization of the mesh takes place in the axes.

Learn more about each of the necessary steps in mesh creation on the following pages:

- Making the grid
- Drawing a subdomain
- Reviewing the subdomains
- Completing the mesh

Previous (Planning your mesh)
Next (Making the grid)