AutoCAD Layer Naming Convention - PlantSectionLayerItemComponent
Example: The chemical doser "tube" would be named - EtCdc"Tube" - 

Plant Section

1. Operator Walkways & Platforms - (Op)

2. OuterWall - (Ow)

3. SedTank - (Sed)

· all manifold pieces including elbows, couplings, and caps - (Man)

· all launder pieces including couplings and caps - (Launder)

· the launder coupling cap, the launder orifice cap, and the chimney stops - (ControlPieces)

· all pipes, caps, and lamella in the modules - (Module)

· all parts associated with drain channel - (Drain)

     4. Flocculator - (Floc)

· Drain components - (Drain)

· All module piping and baffles (Module)

     5. Entrance Tank- Including Chemical Doser parts- (Et)

· Chemical Doser - (Cdc)

     6. Filter - (Fi)

     7. Plant Drain - (Pdrain)

Layer Item

Ex. Channel, Tank, Lamina, Coagtank

· Note only the first letter of the layer item is to be capitalized, for example a Coagulant Tank would receive the layer item “Coagtank” not “CoagTank”

Component

Piping, Valves, Couplings - (Plumbing)

Concrete - (Con)

