AguaClara Demo Plant
Directions of Assembly and Operation (04/2009)
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1.) Be sure that all of the necessary pieces are in the case and be prepared with paper towels (there should be some in the demo plant case outside pocket).
2.) Begin setting up the demo plant before or during the presentation to ensure it is running in time.
3.)  (pic1 -> pic2) Place piece A into B, then B into the stand( D). Then  Fill both tanks of part C with water (preferable warm) and attach C to the top of A.
4.) (pic3 -> pic4) Place two of the H  pieces onto F, and the other H piece onto E.  
Fit E and F together, then fill them with water.
5.) (pic5 -> pic6)  Assemble the valves and tubes snuggly, following the color coding.  Make sure that the valves are closed.  The level at which the alum and clay tubes attach from float control to the rapid mix section is labeled in blue marker (see pic8).  One end of the tube that is labeled RM (for rapid mix) attaches the bottom of the rapid mix section (the fixed vertical tube with several holes, pic8)  and the other is placed in the first “slot” of the floculator (section E of picture 8)
6.) Place 2 teaspoons of Alum in the Alum Source (tank1 of pic1), and 2 tablespoons of clay in the Dirty Water Source (tank2 of pic1).  Stir each tank with the stir stick (pic 7) rinsing it between stirring the different tanks.
7.) Be sure to place a container under the outflow from the lamella (section F from pic3-4)
8.) Open the valves and monitor for leaks, -often leaks may be avoided by tightening the tube-valve attachment.
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